Installation
============

Unpack this ZIP-archive into a new folder, open the web-interface of the
device in your web-browser and log in as administrator.

In the web-interface, select menu item "Backup" in the menu "System" and
navigate to the end of the resulting page "Backup". There you find the
section "Update Device". Click the button "Choose a file..." and choose the
file "rootfs.tar.gz" in the folder that was created aboved, containing the
contents of this ZIP-archive. Then click the button "Update".

The update process can take one to two minutes, depending on the network
throughput, and will be completed by a restart of the device. Be sure to
provide a stable power supply for the device throughout the entire update
process.

For further information, refer to the end of user manual section 10.5.2.15.
